# Version 1.1 | Date 05/26/2022

* Documentation created by Neil Squire / Makers Making Change.

**Minor Modifications by Neil Squire:**

* Changed the length of the hole for the screws so that all buttons can be attached with the same length of screw.
* The width of the countersink of the screw holes were made larger to accommodate screws with wider heads.
* All the depths of the T-Nut inserts were different, some too deep or too shallow, so all were changed to 2.4mm. (T-Nut flush with bottom with some margin)
* All the heights of the mounts were different, and all heights were changed to approx. 9.5mm. (T-Nut flush with top of mount).

# Version 1.0 | Date 01/26/2020

Design created by AT Makers